SO2 sensor (AlphaSense 4-Elec ISB REV 4)

<https://www.isweek.com/product/individual-sensor-board-isb-alphasense-b4-4-electrode-gas-sensors-isb_51.html>

VCC -> VCC -> 6V  
GND -> GND -> GND  
SIG+ -> SIG+ -> A4 (INPUT)  
SIG- -> GND

SainSmart MAX6675 Module + K Type Thermocouple

<https://www.amazon.com/gp/product/B00PVTH4MW/ref=ppx_yo_dt_b_asin_title_o01_s00?ie=UTF8&psc=1>

VCC -> 3.3V

GND -> GND

DO/SO -> A5 (OUTPUT)

CS -> D10 (OUTPUT)

SCK -> D11 (OUTPUT)

Limiting Switch

NO -> GND

NO -> pin\_SDA (INPUT / Digital Read)

NC -> 3.3V

NC -> pin\_SDA (INPUT/ Digital Read)